Bowtie-Chirplet Transform: sea clutter only

Beginning Frequency

Ending Frequency

-500 Hz +500 Hz

-500 Hz +500 Hz