0 100 200 300 400

-50 Hz 0 50 Hz

DIAGONAL SLICE (same as FFT)

Frequency 0 200 400 600 800

-50 Hz 0 50 Hz

OFF DIAGONAL SLICE (through "bowtie")

Average "instantaneous frequency"