Frame 0 (spatial reference frame)

Frame 1 (spatial comparison frame)

Combined frame, in spatial coordinates of frame 0

Different exposures combined into the same coordinate system (domain and range coordinates matched)